NM ID: au613020106003

WOKWI LINK:

<https://wokwi.com/projects/363692710824671233>

ASSIGNMENT CODE:

void setup()

{

pinMode(3, INPUT);

pinMode(13, OUTPUT);

}

void loop()

{

if (digitalRead(3) == HIGH) {

digitalWrite(13, HIGH);

} else {

digitalWrite(13, LOW);

}

delay(10); // Delay a little bit to improve simulation performance

}

ASSIGNMENT SCREESHOT

